When the OUTPUT CTRL pin is tied to ground, the TL494 is operating in single-ended or parallel mode. When

the OUTPUT CTRL pin is tied to VREF, the TL494 is operating in normal push-pull operation.